<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.5.2b.02.18.4756" moduleId="c7c8e292b3beec531de0c51f2576d329">
    <version>4</version>
    <author>Brendan Howell/Dirk van Osterbosch/Lionel Michel</author>
    <title>4 x AAA Battery Mount</title>
    <label>VCC</label>
    <date>2009-10-23</date>
    <tags>
        <tag>Battery</tag>
        <tag>power supply</tag>
        <tag>user part</tag>
    </tags>
    <properties>
        <property name="family">Battery</property>
        <property name="voltage">4.8V</property>
    </properties>
    <description>A 4 x AAA battery pack (4.8 Volts with recharables)</description>
    <views>
        <iconView>
            <layers image="icon/batterypack_2xAA.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/batterypack_4xAAA.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/dc_powersupply.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/battery_pack_mounted_500mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" type="male" name="-">
            <description>negative side</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" legId="connector0leg" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="+">
            <description>positive side</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" legId="connector1leg" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
