<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.4b.10.03.4492" moduleId="Teensy3.0" referenceFile="Teensy 3.0.fzp">
    <author>Fabian Althaus</author>
    <title>Teensy 3.0</title>
    <label>Teensy</label>
    <date>mo jul 15 2013</date>
    <tags>
        <tag>Teensy 3.0</tag>
        <tag>microcontroller</tag>
    </tags>
    <properties>
        <property name="family">microcontroller board (teensy)</property>
        <property name="variant">Teensy 3.0</property>
        <property name="processor">ATmega</property>
        <property name="part number"/>
    </properties>
    <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">The Teensy is a complete USB-based microcontoller development system, in a very small footprint, capable of implementing many types of projects. All programming is done via the USB port. No special programmer is needed, only a standard micro-USB cable and a PC or Macintosh with a USB port.&lt;/p>&lt;/body>&lt;/html></description>
    <views>
        <iconView>
            <layers image="icon/Teensy_3.0_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Teensy_3.0_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Teensy_3.0_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Teensy_3.0_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector type="male" id="connector15" name="3V3">
            <description>3.3V Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector15pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector15pin" layer="schematic" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector15pin" layer="copper0"/>
                    <p svgId="connector15pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector7" name="D6">
            <description>Digital Inpout/Output and PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector7pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector7pin" layer="schematic" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector7pin" layer="copper0"/>
                    <p svgId="connector7pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector16" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector16pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector16pin" layer="schematic" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector16pin" layer="copper0"/>
                    <p svgId="connector16pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector8" name="D7">
            <description>Digital Inpout/Output and RX3</description>
            <views>
                <breadboardView>
                    <p svgId="connector8pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8pin" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8pin" layer="copper0"/>
                    <p svgId="connector8pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector17" name="Program">
            <description>Program</description>
            <views>
                <breadboardView>
                    <p svgId="connector17pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector17pin" layer="schematic" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector17pin" layer="copper0"/>
                    <p svgId="connector17pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector9" name="D8">
            <description>Digital Inpout/Output and TX3</description>
            <views>
                <breadboardView>
                    <p svgId="connector9pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9pin" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9pin" layer="copper0"/>
                    <p svgId="connector9pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector18" name="Reset">
            <description>Reset</description>
            <views>
                <breadboardView>
                    <p svgId="connector18pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector18pin" layer="schematic" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector18pin" layer="copper0"/>
                    <p svgId="connector18pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector19" name="D13">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector19pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector19pin" layer="schematic" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector19pin" layer="copper0"/>
                    <p svgId="connector19pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector20" name="A0/D14">
            <description>Analog Input/Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector20pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector20pin" layer="schematic" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector20pin" layer="copper0"/>
                    <p svgId="connector20pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector21" name="A1/D15">
            <description>Analog Input/Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector21pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector21pin" layer="schematic" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector21pin" layer="copper0"/>
                    <p svgId="connector21pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector22" name="A2/D16">
            <description>Analog Input/Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector22pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector22pin" layer="schematic" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector22pin" layer="copper0"/>
                    <p svgId="connector22pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector23" name="A3/D17">
            <description>Analog Input/Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector23pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector23pin" layer="schematic" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector23pin" layer="copper0"/>
                    <p svgId="connector23pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector24" name="A4/D18">
            <description>Analog Input/Digital I/O - SDA</description>
            <views>
                <breadboardView>
                    <p svgId="connector24pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector24pin" layer="schematic" terminalId="connector24terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector24pin" layer="copper0"/>
                    <p svgId="connector24pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector25" name="A5/D19">
            <description>Analog Input/Digital I/O - SCL</description>
            <views>
                <breadboardView>
                    <p svgId="connector25pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector25pin" layer="schematic" terminalId="connector25terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector25pin" layer="copper0"/>
                    <p svgId="connector25pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector26" name="A6/D20">
            <description>Analog Input/Digital I/O, PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector26pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector26pin" layer="schematic" terminalId="connector26terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector26pin" layer="copper0"/>
                    <p svgId="connector26pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector27" name="A7/D21">
            <description>Analog Input/Digital I/O, PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector27pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector27pin" layer="schematic" terminalId="connector27terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector27pin" layer="copper0"/>
                    <p svgId="connector27pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector28" name="A8/D22">
            <description>Analog Input/Digital I/O, PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector28pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector28pin" layer="schematic" terminalId="connector28terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector28pin" layer="copper0"/>
                    <p svgId="connector28pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector29" name="A9/D23">
            <description>Analog Input/Digital I/O, PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector29pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector29pin" layer="schematic" terminalId="connector29terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector29pin" layer="copper0"/>
                    <p svgId="connector29pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector30" name="3V3">
            <description>+3.3V Input (100mA max)</description>
            <views>
                <breadboardView>
                    <p svgId="connector30pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector30pin" layer="schematic" terminalId="connector30terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector30pin" layer="copper0"/>
                    <p svgId="connector30pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector0" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector0pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector0pin" layer="copper0"/>
                    <p svgId="connector0pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector1" name="D0">
            <description>Digital I/O and RX1</description>
            <views>
                <breadboardView>
                    <p svgId="connector1pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector1pin" layer="copper0"/>
                    <p svgId="connector1pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector10" name="D9">
            <description>Digital I/O, PWM and RX2</description>
            <views>
                <breadboardView>
                    <p svgId="connector10pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10pin" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10pin" layer="copper0"/>
                    <p svgId="connector10pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector2" name="D1">
            <description>Digital I/O and TX1</description>
            <views>
                <breadboardView>
                    <p svgId="connector2pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector2pin" layer="copper0"/>
                    <p svgId="connector2pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector3" name="D2">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector3pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector3pin" layer="schematic" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector3pin" layer="copper0"/>
                    <p svgId="connector3pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector11" name="D10">
            <description>Digital I/O, PWM and TX2</description>
            <views>
                <breadboardView>
                    <p svgId="connector11pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11pin" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector11pin" layer="copper0"/>
                    <p svgId="connector11pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector4" name="D3">
            <description>Digital I/O and PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector4pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector4pin" layer="schematic" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector4pin" layer="copper0"/>
                    <p svgId="connector4pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector12" name="D11">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector12pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector12pin" layer="schematic" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector12pin" layer="copper0"/>
                    <p svgId="connector12pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector5" name="D4">
            <description>Digital I/O and PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector5pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector5pin" layer="schematic" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector5pin" layer="copper0"/>
                    <p svgId="connector5pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector13" name="D12">
            <description>Digital I/O</description>
            <views>
                <breadboardView>
                    <p svgId="connector13pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector13pin" layer="schematic" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector13pin" layer="copper0"/>
                    <p svgId="connector13pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector6" name="D5">
            <description>Digital I/O and PWM</description>
            <views>
                <breadboardView>
                    <p svgId="connector6pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector6pin" layer="schematic" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector6pin" layer="copper0"/>
                    <p svgId="connector6pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector14" name="VBat">
            <description>Voltage Input, use 3V coin cell for real time clock</description>
            <views>
                <breadboardView>
                    <p svgId="connector14pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector14pin" layer="schematic" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector14pin" layer="copper0"/>
                    <p svgId="connector14pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector31" name="AGND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p svgId="connector31pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector31pin" layer="schematic" terminalId="connector31terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector31pin" layer="copper0"/>
                    <p svgId="connector31pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector32" name="Vin">
            <description>3.7V to 5.5V </description>
            <views>
                <breadboardView>
                    <p svgId="connector32pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector32pin" layer="schematic" terminalId="connector32terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector32pin" layer="copper0"/>
                    <p svgId="connector32pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector33" name="A11">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector33pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector33pin" layer="schematic" terminalId="connector33terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector33pin" layer="copper0"/>
                    <p svgId="connector33pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector34" name="A10">
            <description>Analog Input</description>
            <views>
                <breadboardView>
                    <p svgId="connector34pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector34pin" layer="schematic" terminalId="connector34terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector34pin" layer="copper0"/>
                    <p svgId="connector34pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector35" name="AREF">
            <description>Aref</description>
            <views>
                <breadboardView>
                    <p svgId="connector35pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector35pin" layer="schematic" terminalId="connector35terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector35pin" layer="copper0"/>
                    <p svgId="connector35pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector36" name="VUSB">
            <description>VUSB</description>
            <views>
                <breadboardView>
                    <p svgId="connector36pin" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector36pin" layer="schematic" terminalId="connector36terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector36pin" layer="copper0"/>
                    <p svgId="connector36pin" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
    <buses>
        <bus id="GND">
            <nodeMember connectorId="connector16"/>
            <nodeMember connectorId="connector0"/>
        </bus>
        <bus id="VCC">
            <nodeMember connectorId="connector30"/>
            <nodeMember connectorId="connector14"/>
        </bus>
    </buses>
</module>
