<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.15b.02.03.3943" moduleId="LCD-GDM1602K">
    <version>4</version>
    <author>Lionel Michel</author>
    <title>LCD screen</title>
    <label>LCD</label>
    <date>2010-02-10</date>
    <tags>
        <tag>LCD</tag>
        <tag>Liquid Crystal</tag>
        <tag>display</tag>
				<tag>line display</tag>
				<tag>character display</tag>
        <tag>screen</tag>
    </tags>
    <properties>
        <property name="family">LCD Display</property>
        <property name="type">Character</property>
        <property name="pins">16</property>
    </properties>
    <description>A standard character display, usually with 2x16 characters. Comes in many colors.</description>
    <views>
        <iconView>
            <layers image="icon/lcd-GDM1602K.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/lcd-GDM1602K.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/lcd-GDM1602K.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/lcd-GDM1602K.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="keepout"/>
                <layer layerId="soldermask"/>
                <layer layerId="outline"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" name="VSS" type="male">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="VDD" type="male">
            <description>+5V</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector2" name="V0" type="male">
            <description>Contrast adjustment</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                <p layer="copper1" svgId="connector2pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector3" name="RS" type="male">
            <description>H/L Register select signal</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin"/>
                <p layer="copper1" svgId="connector3pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector4" name="R/W" type="male">
            <description>H/L Read/Write signal</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin"/>
                <p layer="copper1" svgId="connector4pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector5" name="E" type="male">
            <description>H/L Enable signal</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pin"/>
                <p layer="copper1" svgId="connector5pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector6" name="DB0" type="male">
            <description>H/L Data bus line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pin"/>
                <p layer="copper1" svgId="connector6pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector7" name="DB1" type="male">
            <description>H/L Data bus line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector7pin"/>
                <p layer="copper1" svgId="connector7pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector8" name="DB2" type="male">
            <description>H/L Data bus line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector8pin"/>
                <p layer="copper1" svgId="connector8pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector9" name="DB3" type="male">
            <description>H/L Data bus line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector9pin"/>
                <p layer="copper1" svgId="connector9pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector10" name="DB4" type="male">
            <description>H/L Data bus line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector10pin"/>
                <p layer="copper1" svgId="connector10pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector11" name="DB5" type="male">
            <description>H/L Data bus line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector11pin"/>
                <p layer="copper1" svgId="connector11pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector12" name="DB6" type="male">
            <description>H/L Data bus line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector12pin"/>
                <p layer="copper1" svgId="connector12pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector13" name="DB7" type="male">
            <description>H/L Data bus line</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector13pin"/>
                <p layer="copper1" svgId="connector13pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector14" name="LED+" type="male">
            <description>LED power supply (Anode)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector14pin"/>
                <p layer="copper1" svgId="connector14pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector15" name="LED-" type="male">
            <description>LED power supply (GND)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector15pin"/>
                <p layer="copper1" svgId="connector15pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>