<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Sensors-IMU3000-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Sensors' IMU3000  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>3-axis I2C programmable gyro.&lt;BR&gt;
Can interface with an I2C accelerometer to provide 6-axis motion information.</description>
<title>IMU3000</title>
<tags>
<tag>IMU3000</tag>
<tag>QFN-24</tag>
</tags>
<properties>
<property name="package">qfn-24</property>
<property name="family">sparkfun Gyroscope</property>
<property name="features">programmable</property>
<property name="interface">I2C</property>
<property name="axis">3</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/QFN-24_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-sensors_imu3000_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-sensors_qfn-24_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/QFN-24_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector8" name="AD0" type="male">
<description>AD0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="AUX_CL" type="male">
<description>AUX_CL</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="AUX_DA" type="male">
<description>AUX_DA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="CLKIN" type="male">
<description>CLKIN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector21" name="CLKOUT" type="male">
<description>CLKOUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector21pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector21pad"/>
</pcbView>
</views>
</connector>
<connector id="connector19" name="CPOUT" type="male">
<description>CPOUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector19pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector19pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector17" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector17pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector17pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="INT" type="male">
<description>INT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="REGOUT" type="male">
<description>REGOUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector22" name="SCL" type="male">
<description>SCL</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector22pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector22pad"/>
</pcbView>
</views>
</connector>
<connector id="connector23" name="SDA" type="male">
<description>SDA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector23pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector23pad"/>
</pcbView>
</views>
</connector>
<connector id="connector12" name="VDD" type="male">
<description>VDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="VLOG" type="male">
<description>VLOG</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id="GND">
<nodeMember connectorId="connector17"/>
<nodeMember connectorId="connector10"/>
</bus>
</buses>
</module>