<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Connectors-IPOD_CONNECTOR_MALE-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' IPOD_CONNECTOR_MALE  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;iPod Male Connector&lt;/b&gt;
This is the connector that will insert into an iPods. Use this connector to gain access to the various iPod pins. Schematic and footprint are not yet production proven. The PCB thickness must be more thin than the standard 0.062 FR4. Spark Fun Electronics SKU : DEV-00633</description>
<title>iPod Male Connector</title>
<tags>
<tag>IPOD_CONNECTOR_MALE</tag>
<tag>IPOD_MALE_CONNECTOR</tag>
</tags>
<properties>
<property name="package">ipod_male_connector</property>
<property name="family">sparkfun iPod</property>
<property name="variant">male</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-connectors_ipod_male_connector_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-connectors_ipod_connector_female_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-connectors_ipod_male_connector_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/IPOD_MALE_CONNECTOR.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector13" name="14" type="male">
<description>14</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector13pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector13pad"/>
</pcbView>
</views>
</connector>
<connector id="connector16" name="17" type="male">
<description>17</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector16pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector16pad"/>
</pcbView>
</views>
</connector>
<connector id="connector17" name="3.3V" type="male">
<description>3.3V</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector17pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector17pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="7" type="male">
<description>7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector20" name="ACC_INDICATOR" type="male">
<description>ACC_INDICATOR</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector20pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector20pad"/>
</pcbView>
</views>
</connector>
<connector id="connector18" name="FW_12V" type="male">
<description>FW_12V</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector18pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector18pad"/>
</pcbView>
</views>
</connector>
<connector id="connector19" name="FW_12V" type="male">
<description>FW_12V</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector19pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector19pad"/>
</pcbView>
</views>
</connector>
<connector id="connector23" name="FW_TPA+" type="male">
<description>FW_TPA+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector23pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector23pad"/>
</pcbView>
</views>
</connector>
<connector id="connector21" name="FW_TPA-" type="male">
<description>FW_TPA-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector21pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector21pad"/>
</pcbView>
</views>
</connector>
<connector id="connector27" name="FW_TPB+" type="male">
<description>FW_TPB+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector27pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector27pad"/>
</pcbView>
</views>
</connector>
<connector id="connector25" name="FW_TPB-" type="male">
<description>FW_TPB-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector25pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector25pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector14" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector14pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector14pad"/>
</pcbView>
</views>
</connector>
<connector id="connector15" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector15pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector15pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector28" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector28pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector28pin" terminalId="connector28terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector28pad"/>
</pcbView>
</views>
</connector>
<connector id="connector29" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector29pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector29pin" terminalId="connector29terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector29pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="LEFT_IN" type="male">
<description>LEFT_IN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="LEFT_OUT" type="male">
<description>LEFT_OUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="RIGHT_IN" type="male">
<description>RIGHT_IN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="RIGHT_OUT" type="male">
<description>RIGHT_OUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector12" name="RX" type="male">
<description>RX</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="SCHROME_OUT" type="male">
<description>SCHROME_OUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="SLUM_OUT" type="male">
<description>SLUM_OUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="TX" type="male">
<description>TX</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
<connector id="connector22" name="USB_5V" type="male">
<description>USB_5V</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector22pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector22pad"/>
</pcbView>
</views>
</connector>
<connector id="connector26" name="USB_D+" type="male">
<description>USB_D+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector26pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector26pad"/>
</pcbView>
</views>
</connector>
<connector id="connector24" name="USB_D-" type="male">
<description>USB_D-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector24pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector24pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="VIDEO_OUT" type="male">
<description>VIDEO_OUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id="FW_12V">
<nodeMember connectorId="connector19"/>
<nodeMember connectorId="connector18"/>
</bus>
<bus id="GND">
<nodeMember connectorId="connector29"/>
<nodeMember connectorId="connector28"/>
<nodeMember connectorId="connector1"/>
<nodeMember connectorId="connector15"/>
<nodeMember connectorId="connector14"/>
<nodeMember connectorId="connector10"/>
<nodeMember connectorId="connector0"/>
</bus>
</buses>
</module>