<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.6.5b.01.02.5717" moduleId="0169a1437c0125d6d12452c99a8c3cc3">
    <version replacedby="SparkFun-DigitalIC-ATMEGA168-">4</version>
    <author>drew</author>
    <title>Atmega 168 TQFP32</title>
    <label>ATmega168 TQFP</label>
    <date>2011-06-17</date>
    <tags>
        <tag>SMD</tag>
    </tags>
    <properties>
        <property name="package">TQFP32-5MM</property>
        <property name="family">/obsolete/Microcontroller</property>
        <property name="editable pin labels">true</property>
        <property name="chip label">ATmega168</property>
        <property name="part number"></property>
    </properties>
    <description>THIS PACKAGE DOES NOT EXIST IN REALITY. ATmel's ever popular 168 in a TQFP package!</description>
    <views>
        <iconView>
            <layers image="icon/Atmega_168_TQFP32_icon.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Atmega_168_TQFP32_breadboard.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Atmega_168_TQFP32_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Atmega_168_TQFP32_pcb.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector15" type="male" name="Pin 16">
            <description>PB4 (PCINT4/MISO)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector15pad"/>
                    <p layer="copper1" svgId="connector15pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="male" name="Pin 8">
            <description>PB7 (PCINT7/XTAL2/TOSC2)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector7pad"/>
                    <p layer="copper1" svgId="connector7pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" type="male" name="Pin 17">
            <description>PB5 (SCK/PCINT5)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector16pad"/>
                    <p layer="copper1" svgId="connector16pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="male" name="Pin 9">
            <description>PD5 (PCINT21/OC0B/T1)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector8pad"/>
                    <p layer="copper1" svgId="connector8pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector17" type="male" name="Pin 18">
            <description>AVCC</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector17pad"/>
                    <p layer="copper1" svgId="connector17pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" type="male" name="Pin 10">
            <description>PD6 (PCINT22/OC0A/AIN0)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector9pad"/>
                    <p layer="copper1" svgId="connector9pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" type="male" name="Pin 19">
            <description>ADC6</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector18pad"/>
                    <p layer="copper1" svgId="connector18pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" type="male" name="Pin 20">
            <description>AREF</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector19pad"/>
                    <p layer="copper1" svgId="connector19pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector20" type="male" name="Pin 21">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector20pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector20pad"/>
                    <p layer="copper1" svgId="connector20pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector21" type="male" name="Pin 22">
            <description>ADC7</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector21pad"/>
                    <p layer="copper1" svgId="connector21pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector22" type="male" name="Pin 23">
            <description>PC0 (ADC0/PCINT8)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector22pad"/>
                    <p layer="copper1" svgId="connector22pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector23" type="male" name="Pin 24">
            <description>PC1 (ACD1/PCINT9)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector23pad"/>
                    <p layer="copper1" svgId="connector23pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector24" type="male" name="Pin 25">
            <description>pC2 (ADC2/PCINT10)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector24pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector24pad"/>
                    <p layer="copper1" svgId="connector24pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector25" type="male" name="Pin 26">
            <description>PC3 (ADC3/PCINT11)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector25pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector25pad"/>
                    <p layer="copper1" svgId="connector25pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector26" type="male" name="Pin 27">
            <description>PC4 (ACD4/SDA/PCINT12)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector26pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector26pad"/>
                    <p layer="copper1" svgId="connector26pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector27" type="male" name="Pin 28">
            <description>PC5 (ADC5/SCL/PCINT13)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector27pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector27pad"/>
                    <p layer="copper1" svgId="connector27pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector28" type="male" name="Pin 29">
            <description>PC6 (RESET/PCINT14)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector28pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector28pin" terminalId="connector28terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector28pad"/>
                    <p layer="copper1" svgId="connector28pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector29" type="male" name="Pin 30">
            <description>PD0 (RXD/PCINT16)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector29pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector29pin" terminalId="connector29terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector29pad"/>
                    <p layer="copper1" svgId="connector29pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector30" type="male" name="Pin 31">
            <description>PD1 (TXD/PCINT17)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector30pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector30pin" terminalId="connector30terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector30pad"/>
                    <p layer="copper1" svgId="connector30pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector31" type="male" name="Pin 32">
            <description>PD2 (INT0/PCINT18)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector31pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector31pin" terminalId="connector31terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector31pad"/>
                    <p layer="copper1" svgId="connector31pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="Pin 1">
            <description>PD3 (PCINT19/OC2B/INT1)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pad"/>
                    <p layer="copper1" svgId="connector0pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="Pin 2">
            <description>PD4 (PCINT20/XCK/T0)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pad"/>
                    <p layer="copper1" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" type="male" name="Pin 11">
            <description>PD7 (PCINT23/AIN1)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector10pad"/>
                    <p layer="copper1" svgId="connector10pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="Pin 3">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pad"/>
                    <p layer="copper1" svgId="connector2pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="male" name="Pin 4">
            <description>VCC</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pad"/>
                    <p layer="copper1" svgId="connector3pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" type="male" name="Pin 12">
            <description>PB0 (PCINT0/CLKO/ICP1)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector11pad"/>
                    <p layer="copper1" svgId="connector11pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="Pin 5">
            <description>GND</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pad"/>
                    <p layer="copper1" svgId="connector4pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" type="male" name="Pin 13">
            <description>PB1 (PCINT1/OC1A)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector12pad"/>
                    <p layer="copper1" svgId="connector12pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="male" name="Pin 6">
            <description>VCC</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pad"/>
                    <p layer="copper1" svgId="connector5pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" type="male" name="Pin 14">
            <description>PB2 (PCINT2/SS/OC1B)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector13pad"/>
                    <p layer="copper1" svgId="connector13pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" type="male" name="Pin 15">
            <description>PB3 (PCINT3/OC2A/MOSI)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector14pad"/>
                    <p layer="copper1" svgId="connector14pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="male" name="Pin 7">
            <description>PB6 (PCINT6/XTAL1/TOSC1)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pad"/>
                    <p layer="copper1" svgId="connector6pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
