<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.4.1b.07.17.4356" moduleId="atlas-sientific_Debugger" referenceFile="atlas-sientific_Debugger.fzp">
 <author>Atlas Scientific </author>
 <title>Debugger</title>
 <label>Debugger</label>
 <date>Thu Jul 25 2013</date>
 <tags/>
 <properties>
  <property name="family">Connector</property>
  <property name="variant">variant 1</property>
  <property name="part number"></property>
 </properties>
 <description>&lt;!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0//EN" "http://www.w3.org/TR/REC-html40/strict.dtd">
&lt;html>&lt;head>&lt;meta name="qrichtext" content="1" />&lt;style type="text/css">
p, li { white-space: pre-wrap; }
&lt;/style>&lt;/head>&lt;body style=" font-family:'MS Shell Dlg 2'; font-size:8.25pt; font-weight:400; font-style:normal;">
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">Need to get all of your Atlas Scientific equipment calibrated and running smoothly in the shortest amount of time?&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-size:8pt;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">This Debugger is specially designed to have its pin outs match up directly with all of the Atlas Scientific Circuits. Just plug it into your bread board and your ready to go.&lt;/span>&lt;/p>
&lt;p style="-qt-paragraph-type:empty; margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px; font-size:8pt;">&lt;br />&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Rapid calibration and debugging&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• 2 different output voltages (3.3 and 5.0)&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Header pins directly line up to any Atlas Scientific Circuits&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• This is the exact device used here at Atlas Scientific to test all of&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">  our sensors&lt;/span>&lt;/p>
&lt;p style=" margin-top:0px; margin-bottom:0px; margin-left:0px; margin-right:0px; -qt-block-indent:0; text-indent:0px;">&lt;span style=" font-size:8pt;">• Works as a simple USB to serial converter when not being used   to calibrate/debug&lt;/span>&lt;/p>&lt;/body>&lt;/html></description>
 <views>
  <iconView>
   <layers image="icon/atlas-sientific_Debugger_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <schematicView>
   <layers image="schematic/atlas-sientific_Debugger_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <breadboardView>
   <layers image="breadboard/atlas-sientific_Debugger_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <pcbView>
   <layers image="pcb/atlas-sientific_Debugger_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector type="male" id="connector0" name="5v">
   <description>Supply 5 Voltage</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper1"/>
     <p svgId="connector0pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="3v">
   <description>Supply 3 Voltage</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper1"/>
     <p svgId="connector1pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="GND">
   <description>Supply Ground</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper1"/>
     <p svgId="connector2pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector3" name="RX">
   <description>Data In</description>
   <views>
    <breadboardView>
     <p svgId="connector3pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector3pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector3pin" layer="copper1"/>
     <p svgId="connector3pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector4" name="TX">
   <description>Data Out</description>
   <views>
    <breadboardView>
     <p svgId="connector4pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector4pin" layer="schematic"/>
    </schematicView>
    <pcbView>
     <p svgId="connector4pin" layer="copper1"/>
     <p svgId="connector4pin" layer="copper0"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <url>https://www.atlas-scientific.com/product_pages/embedded/debugger.html</url>
</module>
