<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Sensors-QRB1114-2">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Sensors' QRB1114  -->
<version>4</version>
<date>2013-02-13</date>
<label>Q</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;PHOTOTRANSISTOR REFLECTIVE OBJECT SENSOR&lt;/b&gt;
&lt;p&gt;
The QRB1113/1114 consists of an infrared emitting diode and an NPN silicon phototransistor mounted side by side on a converging
optical axis in a black plastic housing. The phototransistor responds to radiation from the emitting diode only when a reflective
object passes within its field of view. The area of the optimum response approximates a circle .200 in diameter.
&lt;p&gt;Datasheet: http://www.sparkfun.com/datasheets/Sensors/QRB1114.pdf
&lt;p&gt;MAX RATINGS:
&lt;p&gt;EMITTER
&lt;br&gt;Continuous Forward Current (IF) 50 mA
&lt;br&gt;Reverse Voltage (VR) 5 V
&lt;br&gt;Power Dissipation (PD) 100 mW
&lt;p&gt;SENSOR
&lt;br&gt;Collector-Emitter Voltage (VCEO) 30 V
&lt;br&gt;Emitter-Collector Voltage (VECO) 4.5 V
&lt;br&gt;Collector Current 20 mA
&lt;br&gt;Power Dissipation (PD) 100 mW</description>
<title>PHOTOTRANSISTOR REFLECTIVE OBJECT SENSOR</title>
<tags>
<tag>QRB1114</tag>
<tag>QRB1114-SIDE</tag>
</tags>
<properties>
<property name="package">qrb1114-side</property>
<property name="family">sparkfun Reflective Object Sensor</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-sensors_qrb1114-side_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-sensors_qre1113_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-sensors_qrb1114-side_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-sensors_qrb1114-side_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector0" name="A" type="male">
<description>A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector0pad"/>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="C" type="male">
<description>C</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector1pad"/>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="E" type="male">
<description>E</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pad"/>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="K" type="male">
<description>K</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pad"/>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>