<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='RFID_USB_Reader-v14'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description:&lt;/span&gt; The RFID USB Reader is a simple to use, USB to serial base unit for the ID-2, ID-12, and ID-20 readers. Simply plug a reader into the headers and attach a miniUSB cable. Open a terminal program of your choice at 9600bps 8N1, then scan your 125kHz ID tag and the unique 32-bit ID will be shown on the screen. The unit is based on a FTDI chip and comes with a read LED and buzzer.&lt;/p&gt;


&lt;p&gt;


	This new revision uses SMD headers for the RFID module, and has a solder jumper which allows you to disable or enable the buzzer.&lt;br /&gt;


	&lt;br /&gt;


	&lt;strong&gt;Note: &lt;/strong&gt;This product does not come with the RFID reader. Check below for compatible readers.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Dimensions:&lt;/span&gt; 1.4x1.2x0.57&amp;quot;&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Sensors/ID/RFID_USB_Reader-v14.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Sensors/ID/RFID_USB_Reader-v14Eagl.zip&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.ftdichip.com/FTDrivers.htm&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;USB FTDI Drivers for Linux, MAC, and PC&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;strong&gt;Replaces:&lt;/strong&gt; &lt;a href=&quot;http://www.sparkfun.com/products/8852&quot; target=&quot;_blank&quot;&gt;SEN-08852&lt;/a&gt;&lt;/p&gt;


&lt;p&gt;


	&amp;nbsp;&lt;/p&gt;


&lt;p&gt;


	&amp;nbsp;&lt;/p&gt;


&lt;p&gt;


	&lt;object height=&quot;300&quot; width=&quot;560&quot;&gt;&lt;param name=&quot;movie&quot; value=&quot;http://www.youtube.com/v/2ioDBOOAFvM&amp;amp;hl=en_US&amp;amp;fs=1&amp;amp;rel=0&quot; /&gt;&lt;param name=&quot;allowFullScreen&quot; value=&quot;true&quot; /&gt;&lt;param name=&quot;allowscriptaccess&quot; value=&quot;always&quot; /&gt;&lt;embed allowfullscreen=&quot;true&quot; allowscriptaccess=&quot;always&quot; height=&quot;300&quot; src=&quot;http://www.youtube.com/v/2ioDBOOAFvM&amp;amp;hl=en_US&amp;amp;fs=1&amp;amp;rel=0&quot; type=&quot;application/x-shockwave-flash&quot; width=&quot;560&quot;&gt;&lt;/embed&gt;&lt;/object&gt;&lt;/p&gt;</description>
<title>RFID USB Reader</title>
<url>http://www.sparkfun.com/products/9963</url>
<tags>
<tag>RFID</tag>
<tag>USB</tag>
<tag>Reader</tag>
</tags>
<properties>
<property name='family'>RFID</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/RFID_USB_Reader-v14_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/RFID_USB_Reader-v14_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/RFID_USB_Reader-v14_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/RFID_USB_Reader-v14_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector8' type='male' name='GNDT'>
<description>GNDT</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
<connector id='connector9' type='male' name='CP'>
<description>CP</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
<connector id='connector10' type='male' name='ANT2'>
<description>ANT2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad'/><p layer='copper1' svgId='connector10pad'/></pcbView>
</views>
</connector>
<connector id='connector11' type='male' name='ANT1'>
<description>ANT1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad'/><p layer='copper1' svgId='connector11pad'/></pcbView>
</views>
</connector>
<connector id='connector12' type='male' name='TX-O-RS232'>
<description>TX-O-RS232</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='male' name='TX-O'>
<description>TX-O</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
<connector id='connector14' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad'/><p layer='copper1' svgId='connector14pad'/></pcbView>
</views>
</connector>
<connector id='connector15' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad'/><p layer='copper1' svgId='connector15pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
