<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.4.2b.08.04.4392" moduleId="c7acdd26c5e6355cb2e7e05c0aa975c0PotentiometerModuleID">
    <author>tigoe</author>
    <title>AD5206 Digital Potentiometer</title>
    <label>U</label>
    <date>2010-08-10</date>
    <tags>
        <tag>Digital potentiometer</tag>
        <tag>SPI</tag>
    </tags>
    <properties>
        <property name="family">IC-Poti</property>
    <property name="package">DIP28 [THT]</property>
   <property name="Maximum Resistance" showInLabel="yes">10k&#937;</property>
   <property name="power" showInLabel="yes"></property>
    </properties>
    <description>Digital potentiometer. 6 channels with SPI-compatible interface.</description>
    <views>
        <breadboardView>
            <layers image="breadboard/AD5206_Digital_Potentiometer__1569b6e5e5.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/AD5206_Digital_Potentiometer__1569b6e5e5.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/dip_24_300mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
        <iconView>
            <layers image="icon/AD5206_Digital_Potentiometer__1569b6e5e5.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
    </views>
    <connectors>
        <connector id="connector15" name="B1" type="male">
            <description>Channel 1 voltage low</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" terminalId="connector15terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector15pin"/>
                    <p layer="copper0" svgId="connector15pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" name="CLK" type="male">
            <description>Serial clock</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pin"/>
                    <p layer="copper0" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" name="W1" type="male">
            <description>Channel 1 wiper</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin" terminalId="connector16terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector16pin"/>
                    <p layer="copper0" svgId="connector16pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" name="Vss" type="male">
            <description>Voltage low (usually ground)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector8pin"/>
                    <p layer="copper0" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector17" name="A1" type="male">
            <description>Channel 1 voltage high</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin" terminalId="connector17terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector17pin"/>
                    <p layer="copper0" svgId="connector17pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" name="B5" type="male">
            <description>Channel 5 voltage low</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pin"/>
                    <p layer="copper0" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" name="A2" type="male">
            <description>Channel 2 voltage high</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin" terminalId="connector18terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector18pin"/>
                    <p layer="copper0" svgId="connector18pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" name="W2" type="male">
            <description>Channel 2 wiper</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin" terminalId="connector19terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector19pin"/>
                    <p layer="copper0" svgId="connector19pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector20" name="B2" type="male">
            <description>Channel 2 voltage low</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector20pin" terminalId="connector20terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector20pin"/>
                    <p layer="copper0" svgId="connector20pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector21" name="A4" type="male">
            <description>Channel 4 voltage high</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin" terminalId="connector21terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector21pin"/>
                    <p layer="copper0" svgId="connector21pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector22" name="W4" type="male">
            <description>Channel 4 wiper</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin" terminalId="connector22terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector22pin"/>
                    <p layer="copper0" svgId="connector22pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector23" name="B4" type="male">
            <description>Channel 4 voltage low</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin" terminalId="connector23terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector23pin"/>
                    <p layer="copper0" svgId="connector23pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" name="A6" type="male">
            <description>Channel 6 voltage high</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="W6" type="male">
            <description>Channel 6 wiper</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" name="W5" type="male">
            <description>Channel 5 wiper</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector10pin"/>
                    <p layer="copper0" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" name="B6" type="male">
            <description>Channel 6 voltage low</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" name="A5" type="male">
            <description>Channel 5 voltage high</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" terminalId="connector11terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector11pin"/>
                    <p layer="copper0" svgId="connector11pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" name="Gnd" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" name="B3" type="male">
            <description>Channel 3 voltage low</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" terminalId="connector12terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector12pin"/>
                    <p layer="copper0" svgId="connector12pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" name="CS" type="male">
            <description>Chip Select (active low)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" name="W3" type="male">
            <description>Channel 3 wiper</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" terminalId="connector13terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector13pin"/>
                    <p layer="copper0" svgId="connector13pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" name="Vdd" type="male">
            <description>Voltage high</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" name="A3" type="male">
            <description>Channel 3 voltage high</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" terminalId="connector14terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector14pin"/>
                    <p layer="copper0" svgId="connector14pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" name="SDI" type="male">
            <description>Serial Data In</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pin"/>
                    <p layer="copper0" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
