<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.7.0b.02.01.5801" moduleId="Humidity_and_Temperature_Sensor_RHT03_6">
    <author>Martha Maldonado</author>
    <title>Humidity and Temperature Sensor RHT03</title>
    <label>RHT03</label>
    <date>2012-02-17</date>
    <tags>
        <tag>humedad</tag>
        <tag>humidity</tag>
        <tag>temperatura</tag>
        <tag>temperature</tag>
    </tags>
    <properties>
        <property name="sensing element">Polymer humidity capacitor</property>
        <property name="family">MaxDetect Technology</property>
        <property name="power supply">3.3-5.5V DC</property>
        <property name="output signal">Digital Signal</property>
        <property name="part number"/>
    </properties>
    <description>Digital relative humidity &amp; temperature sensor RHT03</description>
    <views>
        <iconView>
            <layers image="icon/Humidity_and_Temperature_Sensor_RHT03_6.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Humidity_and_Temperature_Sensor_RHT03_6.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/Humidity_and_Temperature_Sensor_RHT03_6.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/Humidity_and_Temperature_Sensor_RHT03_6.svg">
                <layer layerId="copper0"/>
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector type="male" id="connector8" name="Vcc">
            <description>3.3 V - 5.5V DC</description>
            <views>
                <breadboardView>
                    <p svgId="connector8" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector8" layer="schematic" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector8pad" layer="copper0"/>
                    <p svgId="connector8pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector9" name="Data-signal">
            <description>It goes directly connect to the digital signal and also it connects by a 1k ohm resistor with Vcc, It's something like this:

Data-signal -> Digital Signal

                   -> 1K ohm -> Vcc</description>
            <views>
                <breadboardView>
                    <p svgId="connector9" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector9" layer="schematic" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector9pad" layer="copper0"/>
                    <p svgId="connector9pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector10" name="GND 1">
            <description>Ground Connection</description>
            <views>
                <breadboardView>
                    <p svgId="connector10" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector10" layer="schematic" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector10pad" layer="copper0"/>
                    <p svgId="connector10pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
        <connector type="male" id="connector11" name="GND 2">
            <description>Ground connection</description>
            <views>
                <breadboardView>
                    <p svgId="connector11" layer="breadboard"/>
                </breadboardView>
                <schematicView>
                    <p svgId="connector11" layer="schematic" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p svgId="connector11pad" layer="copper0"/>
                    <p svgId="connector11pad" layer="copper1"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
