<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.5b.06.14.6067" moduleId="15719464aa8d63048081b2444ea6d39c">
    <version>4</version>
    <author>www.fritzing.org</author>
    <title>microSD Socket</title>
    <label>U</label>
    <date>2012-05-25</date>
    <tags>
        <tag>uSD</tag>
        <tag>storage</tag>
        <tag>disk</tag>
    </tags>
    <properties>
        <property name="family">Storage Connector</property>
        <property name="type">microSD</property>
        <property name="package">Molex 502774-0891 [SMD]</property>
    </properties>
    <description>Push-push type microSD socket.</description>
    <views>
        <iconView>
            <layers image="icon/microSD-socket.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/microSD-socket.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/microSD-socket.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/microSD-socket-molex-502774-0891.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" type="pad" name="NC" >
            <description>Not connected</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="pad" name="CS" >
            <description>Chip Select</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="pad" name="DI" >
            <description>Digital In (MOSI)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="pad" name="VCC" >
            <description>Power (3.3V)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="pad" name="SCK" >
            <description>Serial Clock</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="pad" name="GND" >
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="pad" name="DO" >
            <description>Digital Out (MISO)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector6pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="pad" name="RSV" >
            <description>Reserved</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector7pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="pad" name="SHIELD" >
            <description>Shield</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector8pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" type="pad" name="SHIELD" >
            <description>Shield</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" type="pad" name="SHIELD" >
            <description>Shield</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector10pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" type="pad" name="SHIELD" >
            <description>Shield</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector11pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
  <buses>
    <bus id="shield">
      <nodeMember connectorId="connector8"/>
      <nodeMember connectorId="connector9"/>
      <nodeMember connectorId="connector10"/>
      <nodeMember connectorId="connector11"/>
    </bus>
  </buses>
</module>
