<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.4b.04.10.5970" moduleId="S1133">
    <version>4</version>
    <author>Nikos Vallianos</author>
    <title>S1133 Si Photodiode</title>
    <label>P</label>
    <date>2012-04-20</date>
    <tags>
        <tag>Photodiode</tag>
        <tag>S1133</tag>
        <tag>photometer</tag>
    </tags>
    <properties>
        <property name="package">8mm Ceramic [THT]</property>
        <property name="family">Photodiode</property>
        <property name="current"></property>
        <property name="leg">yes</property>
        <property name="color">UV to IR (320-730nm)</property>
        <property name="part number"></property>
    </properties>
    <description>S1133 photodiode with low dark current by Hamamatsu.</description>
    <views>
        <iconView>
            <layers image="icon/S1133_Si_Photodiode_Icon.svg">
                <layer layerId="breadboard"/>
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/S1133_Si_Photodiode_BB.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/S1133_Si_Photodiode_Sch.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/S1133_Si_Photodiode_PCB.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" type="male" name="cathode">
            <description>cathode pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0leg" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pad"/>
                    <p layer="copper1" svgId="connector0pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="anode">
            <description>anode pin</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1leg" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pad"/>
                    <p layer="copper1" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
