<?xml version='1.0' encoding='UTF-8'?><module fritzingVersion='0.4.2b.07.24.4368' moduleId='fd1b41f61d75a154da35b6f6bd5cca72'>
     <version replacedby='Arduino-Pro-Mini-v13'>4</version>
     <author>Lionel Michel</author>
    <title>Arduino Mini Pro</title>
    <label>Arduino Mini Pro</label>
    <date>2010-07-27</date>
    <tags>
        <tag>Arduino</tag>
        <tag>Arduino Mini Pro</tag>
        <tag>Sparkfun</tag>
    </tags>
    <properties>
        <property name='family'>/obsolete/Microcontroller Board (Arduino)</property>
        <property name='processor'>ATmega</property>
        <property name='variant'>Arduino Pro Mini</property>
    </properties>
    <description>The Arduino Pro Mini is a microcontroller board based on the ATmega168. It has 14 digital input/output pins (of which 6 can be used as PWM outputs), 6 analog inputs, an on-board resonator, a reset button, and holes for mounting pin headers. A six pin header can be connected to an FTDI cable or Sparkfun breakout board to provide USB power and communication to the board.</description>
    <views>
        <iconView>
            <layers image='icon/Arduino_Mini_Prod5.svg'>
                <layer layerId='icon'/>
            </layers>
        </iconView>
        <schematicView>
            <layers image='schematic/Arduino_Mini_Prod5.svg'>
                <layer layerId='schematic'/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image='pcb/Arduino_Mini_Prod5.svg'>
                <layer layerId='copper0'/>
                <layer layerId='silkscreen'/>
                <layer layerId='copper1'/>
            </layers>
        </pcbView>
        <breadboardView>
            <layers image='breadboard/Arduino_Mini_Proc8.svg'>
                <layer layerId='breadboard'/>
            </layers>
        </breadboardView>
    </views>
    <connectors>
        <connector id='connector15' name='BLK' type='female' replacedby='GND'>
            <description>blk</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector15pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector15pin'/>
                    <p layer='copper0' svgId='connector15pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector7' name='A2' type='female' replacedby='A2'>
            <description>Analog Input 2</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector7pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector7pin'/>
                    <p layer='copper0' svgId='connector7pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector16' name='GND' type='female' replacedby='GND'>
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector16pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector16pin' terminalId='connector16terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector16pin'/>
                    <p layer='copper0' svgId='connector16pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector8' name='A3' type='female' replacedby='A3'>
            <description>Analog Input 3</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector8pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector8pin'/>
                    <p layer='copper0' svgId='connector8pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector17' name='VCC' type='female' replacedby='VCC'>
            <description>Regulated power supply (3.3 or 5V)</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector17pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector17pin' terminalId='connector17terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector17pin'/>
                    <p layer='copper0' svgId='connector17pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector9' name='A4' type='female' replacedby='A4'>
            <description>Analog Input 4</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector9pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector9pin'/>
                    <p layer='copper0' svgId='connector9pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector18' name='D0' type='female' replacedby='D0/TX'>
            <description>Digital I/O 0</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector18pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector18pin' terminalId='connector18terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector18pin'/>
                    <p layer='copper0' svgId='connector18pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector19' name='D1' type='female' replacedby='D1/RX'>
            <description>Digital I/O 1</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector19pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector19pin' terminalId='connector19terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector19pin'/>
                    <p layer='copper0' svgId='connector19pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector20' name='GRN' type='female' replacedby='GND'>
            <description>GRN</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector20pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector20pin' terminalId='connector20terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector20pin'/>
                    <p layer='copper0' svgId='connector20pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector21' name='D1' type='female' replacedby='D1/RX'>
            <description>Digital I/O 1</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector21pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector21pin' terminalId='connector21terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector21pin'/>
                    <p layer='copper0' svgId='connector21pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector22' name='D0' type='female' replacedby='D0/TX'>
            <description>Digital I/O 0</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector22pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector22pin' terminalId='connector22terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector22pin'/>
                    <p layer='copper0' svgId='connector22pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector23' name='RST' type='female' replacedby='RESET'>
            <description>Reset</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector23pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector23pin' terminalId='connector23terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector23pin'/>
                    <p layer='copper0' svgId='connector23pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector24' name='GND' type='female' replacedby='GND'>
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector24pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector24pin' terminalId='connector24terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector24pin'/>
                    <p layer='copper0' svgId='connector24pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector25' name='D2' type='female' replacedby='D2'>
            <description>Digital I/O 2</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector25pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector25pin' terminalId='connector25terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector25pin'/>
                    <p layer='copper0' svgId='connector25pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector26' name='D3' type='female' replacedby='D3 PWM'>
            <description>Digital I/O 3</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector26pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector26pin' terminalId='connector26terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector26pin'/>
                    <p layer='copper0' svgId='connector26pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector27' name='D4' type='female' replacedby='D4'>
            <description>Digital I/O 4</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector27pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector27pin' terminalId='connector27terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector27pin'/>
                    <p layer='copper0' svgId='connector27pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector28' name='D5' type='female' replacedby='D5 PWM'>
            <description>Digital I/O 5</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector28pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector28pin' terminalId='connector28terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector28pin'/>
                    <p layer='copper0' svgId='connector28pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector29' name='D6' type='female' replacedby='D6 PWM'>
            <description>Digital I/O 6</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector29pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector29pin' terminalId='connector29terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector29pin'/>
                    <p layer='copper0' svgId='connector29pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector30' name='D7' type='female' replacedby='D7'>
            <description>Digital I/O 7</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector30pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector30pin' terminalId='connector30terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector30pin'/>
                    <p layer='copper0' svgId='connector30pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector31' name='D8' type='female' replacedby='D8'>
            <description>Digital I/O 8</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector31pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector31pin'/>
                    <p layer='copper0' svgId='connector31pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector32' name='D9' type='female' replacedby='D9 PWM'>
            <description>Digital I/O 9</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector32pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector32pin'/>
                    <p layer='copper0' svgId='connector32pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector1' name='D10' type='female' replacedby='D10 PWM/SS'>
            <description>Digital I/O 10</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector1pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector1pin' terminalId='connector1terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector1pin'/>
                    <p layer='copper0' svgId='connector1pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector2' name='D11' type='female' replacedby='D11 PWM/MOSI'>
            <description>Digital I/O 11</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector2pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector2pin' terminalId='connector2terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector2pin'/>
                    <p layer='copper0' svgId='connector2pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector10' name='A5' type='female' replacedby='A5'>
            <description>Analog Input 5</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector10pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector10pin'/>
                    <p layer='copper0' svgId='connector10pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector3' name='D12' type='female' replacedby='D12/MISO'>
            <description>Digital I/O 12</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector3pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector3pin' terminalId='connector3terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector3pin'/>
                    <p layer='copper0' svgId='connector3pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector11' name='VCC' type='female' replacedby='VCC'>
            <description>Regulated power supply (3.3 or 5V)</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector11pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector11pin'/>
                    <p layer='copper0' svgId='connector11pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector4' name='D13' type='female' replacedby='D13/SCK'>
            <description>Digital I/O 13</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector4pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector4pin' terminalId='connector4terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector4pin'/>
                    <p layer='copper0' svgId='connector4pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector12' name='RST' type='female' replacedby='RESET'>
            <description>Reset</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector12pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector12pin'/>
                    <p layer='copper0' svgId='connector12pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector5' name='A0' type='female' replacedby='A0'>
            <description>Analog Input 0</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector5pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector5pin' terminalId='connector5terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector5pin'/>
                    <p layer='copper0' svgId='connector5pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector13' name='GND' type='female' replacedby='GND'>
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector13pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector13pin'/>
                    <p layer='copper0' svgId='connector13pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector6' name='A1' type='female' replacedby='A1'>
            <description>Analog Input 1</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector6pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector6pin'/>
                    <p layer='copper0' svgId='connector6pin'/>
                </pcbView>
            </views>
        </connector>
        <connector id='connector14' name='RAW' type='female' replacedby='RAW'>
            <description>Raw power (unregulated)</description>
            <views>
                <breadboardView>
                    <p layer='breadboard' svgId='connector14pin'/>
                </breadboardView>
                <schematicView>
                    <p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/>
                </schematicView>
                <pcbView>
                    <p layer='copper1' svgId='connector14pin'/>
                    <p layer='copper0' svgId='connector14pin'/>
                </pcbView>
            </views>
        </connector>
    </connectors>
    <buses>
		<bus id='GND'>
			<nodeMember connectorId='connector13'/>
			<nodeMember connectorId='connector24'/>
			<nodeMember connectorId='connector16'/>
		</bus>
		<bus id='VCC'>
			<nodeMember connectorId='connector11'/>
			<nodeMember connectorId='connector17'/>
		</bus>
		<bus id='RST'>
			<nodeMember connectorId='connector12'/>
			<nodeMember connectorId='connector23'/>
		</bus>
		<bus id='RX'>
			<nodeMember connectorId='connector22'/>
			<nodeMember connectorId='connector18'/>
		</bus>
		<bus id='TX'>
			<nodeMember connectorId='connector21'/>
			<nodeMember connectorId='connector19'/>
		</bus>
	</buses>
</module>