<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.7b.08.26.3377" moduleId="1000ABDD10012">
    <version replacedby="2010BBCD20113">2</version>
    <title>Basic Photo-Resistor (Photocell)</title>
    <label>R</label>
    <date>2008-09-25</date>
    <tags>
        <tag>LDR</tag>
        <tag>light dependent resistor</tag>
        <tag>photocell</tag>
        <tag>light sensor</tag>
        <tag>sensor</tag>
        <tag>Fritzing core</tag>
    </tags>
    <properties>
        <property name="resistance@ dark">300 kOhms@ 10 seconds</property>
        <property name="family">obsolete Photo-Resistor</property>
        <property name="resistance@ luminance">16 kOhms@ 10 lux</property>
    <property name="package">THT</property></properties>
    <description>A generic light dependent resistor</description>
    <views>
        <iconView>
            <layers image="icon/basic_ldr.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/basic_ldr.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/ldr.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/axial_lay_300mil.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" name="pin 0" type="male">
            <description>pin0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="pin 1" type="male">
            <description>pin1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>