<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion="0.3.15b.02.03.3943" moduleId="alps-starter-pot9mm" referenceFile="alps-starter-pot9mm.fzp">
 <version>5</version>
 <author>f.althaus</author>
 <title>Rotary Potentiometer (Small)</title>
 <label>R</label>
 <date>Aug 19 2013</date>
 <tags>
  <tag>potentiometer</tag>
  <tag>poti</tag>
  <tag>adjustable</tag>
  <tag>resistor</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">potentiometer</property>
  <property name="type">Rotary Shaft Potentiometer</property>
  <property name="Maximum Resistance" showInLabel="yes">100k&#937;</property>
  <property name="Track">Linear</property>
    <property showInLabel="yes" name="power"></property>
  <property name="size">Rotary - 9mm</property>
  <property name="part number"></property>
 <property name="package">THT</property>
 </properties>
  <taxonomy>discreteParts.resistors.adjustable.potentiometer</taxonomy>
 <description>A rotary adjustable resistor (potentiometer).</description>
 <views>
  <iconView>
   <layers image="icon/starter-poti-small_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <schematicView>
   <layers image="schematic/basic_poti.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/alps-starter-pot9mm_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
    <layer layerId="copper1"/>
   </layers>
  </pcbView>
  <breadboardView>
   <layers image="breadboard/starter-poti-small_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
 </views>
 <connectors>
  <connector type="male" id="connector0" name="leg1">
   <description>leg1</description>
   <views>
    <breadboardView>
     <p svgId="connector0pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector0pin" layer="schematic" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector0pin" layer="copper0"/>
     <p svgId="connector0pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector1" name="wiper">
   <description>wiper</description>
   <views>
    <breadboardView>
     <p svgId="connector1pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector1pin" layer="schematic" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector1pin" layer="copper0"/>
     <p svgId="connector1pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
  <connector type="male" id="connector2" name="leg2">
   <description>leg2</description>
   <views>
    <breadboardView>
     <p svgId="connector2pin" layer="breadboard"/>
    </breadboardView>
    <schematicView>
     <p svgId="connector2pin" layer="schematic" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p svgId="connector2pin" layer="copper0"/>
     <p svgId="connector2pin" layer="copper1"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>
