<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.6b.08.14.3340" moduleId="SMDCrystalModuleID">
<version>4</version>
    <author>Fritzing Core Team</author>
    <title>Crystal</title>
    <label>XTAL</label>
    <date>20101-12-07</date>
    <tags>
        <tag>clock</tag>
        <tag>crystal</tag>
        <tag>quartz</tag>
        <tag>oscillator</tag>
	<tag>piezoelectric</tag>
    <tag>SMD</tag></tags>
    <properties>
        <property name="family">oscillator</property>
        <property name="type">crystal</property>
        <property name="frequency" showInLabel="yes">16 Mhz</property>
    <property name="package">SMD</property></properties>
    <description>Crystal</description>
    <views>
        <iconView>
            <layers image="icon/crystal.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/crystal_leg.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <pcbView>
            <layers image="pcb/SMD_crystal_HC49.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
        <schematicView>
            <layers image="schematic/crystal.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
    </views>
    <connectors>
        <connector id="connector0" name="pin 0" type="male">
            <description>pin 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"  legId="connector0leg" />
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="pin 1" type="male">
            <description>pin 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"  legId="connector1leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>