<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.17b.04.07.4081" moduleId="f0d627984e1614e5c1c797471f529619">
    <version>4</version>
    <author>Lionel Michel</author>
    <title>BASIC Stamp 2pe</title>
    <label>BS</label>
    <date>2010-04-08</date>
    <tags>
        <tag>Basic Stamp 2</tag>
        <tag>Parallax</tag>
    </tags>
    <properties>
        <property name="family">Microcontroller Board (Basic Stamp)</property>
        <property name="processor">PBASIC</property>
        <property name="variant">Basic Stamp 2pe</property>
    </properties>
    <description>The BASIC Stamp 2pe serves as the brains inside of electronics projects and applications that require a programmable microcontroller. It is able to control and monitor timers, keypads, motors, sensors, switches, relays, lights, and more. Programming is performed in an easy-to-learn language called PBASIC.</description>
    <views>
        <iconView>
            <layers image="icon/BASIC_Stamp_2pe.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/BASIC_Stamp_2pe.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/BASIC_Stamp_2pe.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/dip_24_600mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="keepout"/>
                <layer layerId="soldermask"/>
                <layer layerId="outline"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector15" name="P11" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin" terminalId="connector15terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector15pin"/>
                <p layer="copper1" svgId="connector15pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector7" name="P3" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin" terminalId="connector7terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector7pin"/>
                <p layer="copper1" svgId="connector7pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector16" name="P12" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin" terminalId="connector16terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector16pin"/>
                <p layer="copper1" svgId="connector16pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector8" name="P4" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin" terminalId="connector8terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector8pin"/>
                <p layer="copper1" svgId="connector8pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector17" name="P13" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin" terminalId="connector17terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector17pin"/>
                <p layer="copper1" svgId="connector17pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector9" name="P5" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector9pin"/>
                <p layer="copper1" svgId="connector9pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector18" name="P14" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin" terminalId="connector18terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector18pin"/>
                <p layer="copper1" svgId="connector18pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector19" name="P15" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin" terminalId="connector19terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector19pin"/>
                <p layer="copper1" svgId="connector19pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector20" name="VDD" type="male">
            <description>5-volt DC input/output</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector20pin" terminalId="connector20terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector20pin"/>
                <p layer="copper1" svgId="connector20pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector21" name="RES" type="male">
            <description>Reset input/output</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector21pin" terminalId="connector21terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector21pin"/>
                <p layer="copper1" svgId="connector21pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector22" name="VSS" type="male">
            <description>System ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector22pin" terminalId="connector22terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector22pin"/>
                <p layer="copper1" svgId="connector22pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector23" name="VIN" type="male">
            <description>Unregulated power in: accepts 5.5 - 12 VDC (7.5 recommended)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector23pin" terminalId="connector23terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector23pin"/>
                <p layer="copper1" svgId="connector23pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector0" name="SOUT" type="male">
            <description>Serial Out</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="SIN" type="male">
            <description>Serial In</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector10" name="P6" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector10pin"/>
                <p layer="copper1" svgId="connector10pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector2" name="ATN" type="male">
            <description>Attention: connects to PC serial port DTR pin for programming.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                <p layer="copper1" svgId="connector2pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector3" name="VSS" type="male">
            <description>System ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin"/>
                <p layer="copper1" svgId="connector3pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector11" name="P7" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" terminalId="connector11terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector11pin"/>
                <p layer="copper1" svgId="connector11pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector4" name="P0" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin"/>
                <p layer="copper1" svgId="connector4pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector12" name="P8" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" terminalId="connector12terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector12pin"/>
                <p layer="copper1" svgId="connector12pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector13" name="P9" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" terminalId="connector13terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector13pin"/>
                <p layer="copper1" svgId="connector13pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector5" name="P1" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pin"/>
                <p layer="copper1" svgId="connector5pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector6" name="P2" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin" terminalId="connector6terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pin"/>
                <p layer="copper1" svgId="connector6pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector14" name="P10" type="male">
            <description>General-purpose I/O pins: each can source and sink 30 mA.</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" terminalId="connector14terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector14pin"/>
                <p layer="copper1" svgId="connector14pin"/></pcbView>
            </views>
        </connector>
    </connectors>
            <buses>
    	<bus id="ground">
      		<nodeMember connectorId="connector3"/>
      		<nodeMember connectorId="connector22"/>
    	</bus>
    </buses>
</module>