<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='HMC5883L_Breakout-v11'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>This is a breakout board for Honeywell&apos;s HMC5883, a 3-axis digital compass. Communication with the HMC5883 is simple and all done through an I2C interface. There is no on-board regulator, so a regulated voltage of 2.16-3.6VDC should be supplied.



The breakout board includes the HMC584843 sensor and all filtering capacitors as shown. The power and 2-wire interface pins are all broken out to a 0.1&quot; pitch header.



Features:



   * Simple I2C interface

   * 2.16 to 3.6VDC supply range

   * Low current draw

   * 5 milli-gauss resolution



Dimensions: 0.7x0.7&quot; (17.78x17.78mm) </description>
<title>Triple Axis Magnetometer - HMC5883 Breakout</title>
<url>N/A</url>
<tags>
<tag>Triple</tag>
<tag>Axis</tag>
<tag>Magnetometer</tag>
<tag>Magnet</tag>
<tag>Compass</tag>
</tags>
<properties>
<property name='family'>Magnetometer Breakout</property>
<property name='Tilt Compensated'>No</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/HMC5883L_Breakout-v11_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/HMC5883L_Breakout-v11_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/HMC5883L_Breakout-v11_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/HMC5883L_Breakout-v11_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector6' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector6pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector6pad'/><p layer='copper1' svgId='connector6pad'/></pcbView>
</views>
</connector>
<connector id='connector7' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector7pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector7pad'/><p layer='copper1' svgId='connector7pad'/></pcbView>
</views>
</connector>
<connector id='connector8' type='male' name='SDA'>
<description>SDA</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
<connector id='connector9' type='male' name='SCL'>
<description>SCL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
