<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Electromechanical-STAND-OFF-TIGHT">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Electromechanical' STAND-OFF TIGHT -->
<version>4</version>
<date>2013-02-13</date>
<label>JP</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;#4 Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
<title>#4 Stand Off</title>
<tags>
<tag>STAND-OFF-TIGHT</tag>
<tag>TIGHT</tag>
<tag>STAND-OFF</tag>
</tags>
<properties>
<property name="package">stand-off-tight</property>
<property name="family">sparkfun Stand off</property>
<property name="variant">tight</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-electromechanical_stand-off-tight_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-electromechanical_stand-off_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-electromechanical_stand-off-tight_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-electromechanical_stand-off-tight_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
</connectors>
</module>