<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-PowerIC-MAX98300-ETA+">
<!-- generated from Sparkfun Eagle Library 'SparkFun-PowerIC' MAX98300 ETA+ -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;Mono 2.6W Class D Amplifier&lt;/b&gt;&lt;p&gt;

Datasheet: &lt;a href=http://datasheets.maxim-ic.com/en/ds/MAX98300.pdf&gt;http://datasheets.maxim-ic.com/en/ds/MAX98300.pdf&lt;/a&gt;&lt;p&gt;

The MAX98300 mono 2.6W Class D amplifier provides
Class AB audio performance with Class D efficiency.
This device offers five selectable gain settings (0dB,
3dB, 6dB, 9dB, and 12dB) set by a single gain-select
input (GAIN).
Active emissions-limiting edge-rate and overshoot control
circuitry greatly reduces EMI. A patented filterless
spread-spectrum modulation scheme eliminates the need
for output filtering found in traditional Class D devices.
These features reduce application component count.
The MAX98300 industry-leading 0.78mA at 3.7V (1.1mA
at 5V) quiescent current extends battery life in portable
applications.
The MAX98300 is available in an 8-pin TDFN-EP (2mm
x 2mm x 0.8mm) and a 9-bump (1.2mm x 1.2mm) WLP.
Both packages are specified over the extended -40NC to
+85NC temperature range.</description>
<title>Mono 2.6W Class D Amplifier</title>
<tags>
<tag>MAX98300</tag>
<tag>ETA+</tag>
<tag>8-TDFN-EP</tag>
</tags>
<properties>
<property name="package">8-tdfn-ep</property>
<property name="family">sparkfun Audio Amplifier</property>
<property name="chip">max98300</property>
<property name="power">2.6W (Class D)</property>
<property name="variant">eta+</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-poweric_8-tdfn-ep_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-poweric_max98300_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-poweric_8-tdfn-ep_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-poweric_8-tdfn-ep_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector3" name="GAIN" type="male">
<description>GAIN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="IN+" type="male">
<description>IN+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="IN-" type="male">
<description>IN-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="OUT+" type="male">
<description>OUT+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="OUT-" type="male">
<description>OUT-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="SHDN" type="male">
<description>SHDN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="VDD" type="male">
<description>VDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id="GND">
<nodeMember connectorId="connector8"/>
<nodeMember connectorId="connector4"/>
</bus>
</buses>
</module>