<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.4.0b.06.21.4282" moduleId="7segment20cat">
    <version>4</version>
    <author>Stefan Hermann</author>
    <title>7 Segment Display</title>
    <label>7 Segment</label>
    <date>2011-08-4</date>
    <tags>
        <tag>fritzing core</tag>
        <tag>led</tag>
        <tag>display</tag>
        <tag>7</tag>
        <tag>segment</tag>
    </tags>
    <properties>
        <property name="family">Character Display</property>
        <property name="type">7 Segment</property>
        <property name="size">20mm</property>
        <property name="common">cathode</property>
    </properties>
    <description>7 Segment Display with common cathode.</description>
    <views>
        <iconView>
            <layers image="icon/7segment.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/7segment_20,32.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/7segment_20,32_cat.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/7segment_20,32.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>

        <connector id="connector1" name="Segment A" type="male">
            <description>Segment A</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector2" name="Segment F" type="male">
            <description>Segment F</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pin"/>
                    <p layer="copper0" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector3" name="common cathode" type="male">
            <description>common cathode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pin"/>
                    <p layer="copper0" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector4" name="Segment E" type="male">
            <description>Segment E</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pin"/>
                    <p layer="copper0" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>

				<connector id="connector5" name="common cathode" type="male">
            <description>common cathode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector5pin"/>
                    <p layer="copper0" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector9" name="Segment DP" type="male">
            <description>Segment DP</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin" terminalId="connector9terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector9pin"/>
                    <p layer="copper0" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>



        <connector id="connector10" name="Segment D" type="male">
            <description>Segment D</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin" terminalId="connector10terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector10pin"/>
                    <p layer="copper0" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector11" name="common cathode" type="male">
            <description>common cathode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin" terminalId="connector11terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector11pin"/>
                    <p layer="copper0" svgId="connector11pin"/>
                </pcbView>
            </views>
        </connector>

				<connector id="connector12" name="common cathode" type="male">
            <description>common cathode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin" terminalId="connector12terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector12pin"/>
                    <p layer="copper0" svgId="connector12pin"/>
                </pcbView>
            </views>
        </connector>

        <connector id="connector13" name="Segment G" type="male">
            <description>Segment G</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin" terminalId="connector13terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector13pin"/>
                    <p layer="copper0" svgId="connector13pin"/>
                </pcbView>
            </views>
        </connector>


        <connector id="connector14" name="Segment B" type="male">
            <description>Segment B</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin" terminalId="connector14terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector14pin"/>
                    <p layer="cathodecopper0" svgId="connector14pin"/>
                </pcbView>
            </views>
        </connector>

        	<connector id="connector16" name="common cathode" type="male">
	            <description>common cathode</description>
	            <views>
	                <breadboardView>
	                    <p layer="breadboard" svgId="connector16pin" terminalId="connector16terminal"/>
	                </breadboardView>
	                <schematicView>
	                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
	                </schematicView>
	                <pcbView>
	                    <p layer="copper1" svgId="connector16pin"/>
	                    <p layer="copper0" svgId="connector16pin"/>
	                </pcbView>
	            </views>
	        </connector>
        
    </connectors>
    <buses>
      <bus id="cathode">
       <nodeMember connectorId="connector3"/>
       <nodeMember connectorId="connector5"/>
			 <nodeMember connectorId="connector11"/>
			 <nodeMember connectorId="connector16"/>
      </bus>
    </buses>
</module>